\input lpg-defs
%
% Tables for LPG.TEX
%

\let\hf=\hfill

\noncenteredtables

\def\tablestrut{\vrule height 13pt depth 2pt width 0pt}

\begintable
{\bf Fuel Tank}\hf			|\hf Quan| Price| Cost \crthick
LPG Motor Fuel Tank\hf			|\hf 1	|\hf	|\hf 400.00 \nr
{\bf Cost:}\hf				|	|	|\hf{ 400.00} \endtable

\vskip\parskip

\begintable
{\bf Major Components}\hf		|\hf Quan| Price| Cost \crthick
Filler Valve Assembly\hf		|\hf 1	|\hf	|\hf 45.00 \nr
Filter/Shutoff, Impco VFF30\hf		|\hf 1	|\hf	|\hf 56.50 \nr
Converter/Regulator, Impco Model L\hf	|\hf 1	|\hf	|\hf 110.00 \nr
Carburetor, Impco CA125\hf		|\hf 1	|\hf	|\hf 67.00 \nr
CI-28 Air Filter Cover\hf		|\hf 1	|\hf	|\hf 9.44 \nr
K\&N Air Filter\hf			|\hf 1	|\hf 	|\hf 13.00 \nr
{\bf Cost:}\hf				|	|	|\hf{\bf 300.94} \endtable

\vskip\parskip

\begintable
{\bf Hose; Quan. is length in feet}\hf|\hf Quan	| Price	| Cost \crthick
LPG Hose, \#6\hf			|\hf 14	|\hf 2.54|\hf 35.56 \nr
LPG Hose, \#8\hf			|\hf 4	|\hf 3.32|\hf 13.28 \nr
LPG Hose, \#4\hf			|\hf 4	|\hf 2.64|\hf 10.56 \nr
Vapor Hose \hf				|\hf 2	|\hf 3.68|\hf 7.36 \nr
Vacuum Hose\hf				|\hf 3	|\hf .38 |\hf 1.14 \nr
{\bf Total Cost:}\hf			|	|	|\hf{\bf 67.90} \endtable

\vskip\parskip

\begintable
{\bf Connectors and Misc. Hardware}\hf	|\hf Quan	| Price	| Cost \crthick
90\degree\ Elbow, \#6 Hose\hf		|\hf 4	|\hf 6.50|\hf 26.00 \nr
45\degree\ Elbow, \#6 Hose\hf		|\hf 1	|\hf 	|\hf 1.28 \nr
Straight Connector, \#8 Hose\hf		|\hf 2	|\hf 3.28|\hf 3.56 \nr
Straight Connector, \#4 Hose\hf		|\hf 2	|\hf 1.84|\hf 3.68 \nr
Male Connector \hf			|\hf 2	|\hf .60 |\hf 1.20 \nr
Brass Elbow\hf				|\hf 2	|\hf 1.86|\hf 3.72 \nr
Zinc Hose Elbow (for vapor hose)\hf	|\hf 1	|\hf	|\hf 1.44 \nr
Male Connector (for crankcase vent)\hf	|\hf 1	|\hf	|\hf 1.34 \nr
Water Hose ``Y''\hf			|\hf 2	|\hf 1.98|\hf 3.96 \nr
{\bf Cost:}\hf				|	|	|\hf{\bf 46.18} \endtable

\vskip\parskip

\begintable
{\bf ``Gas Can'' and spares}\hf		|\hf Quan	| Price	| Cost \crthick
Acme 1-$3\over4$" Connector\hf		|\hf 1	|\hf	|\hf 33.78 \nr
Portable LPG Cylinder, 5 gallon\hf	|\hf 1	|\hf	|\hf 27.61 \nr
Hose Set (2 connectors, 3 ft hose)\hf	|\hf 1	|\hf	|\hf 10.00 \nr
O-rings\hf				|\hf 3	|\hf 1.00|\hf 3.00 \cr
{\bf Cost:}\hf				|	|	|\hf{\bf 74.39} \endtable

\begintable
{\bf Total System Cost}\hf		|\hf \crthick
Motor Fuel Tank, 20 gal.\hf		|\hf 400.00 \nr
Major Components\hf			|\hf 300.94 \nr
Hoses\hf				|\hf 67.90 \nr
Connectors \& Misc.\hf			|\hf 46.18 \nr
Gas Can System\hf			|\hf 74.39 \nr
{\bf Cost:}\hf				|\hf{\bf 889.41} \endtable


\bye
